BENDER COMTRAXX® COM465IP / COM465DP / CP700 / CP907 / CP900
Changelog

IMPORTANT: 
All COMTRAXX® devices in a system must be updated.
It is necessary that one COMTRAXX® device operate as BCOM-proxy in each BCOM-subsystem.
If you have display problems in the browser after an update, first empty the browser cache.
V4.0.2 is the new basic version for all upcoming updates. This means that the COMTRAXX® device must always be updated to V4.0.2 before a higher update can be installed.

.................................................................................

V4.0.2
Date: March 2020 | Device: COM465IP / COM465DP / CP700 / CP907 / CP900

Note: The Silverlight application has been completely removed. The new visualization has been integrated into the HTML application.

Two system views: representation by interfaces / representation by subsystems
New internal addressing: Each interface has its own address space
Modbus device integration:
- Modbus channel templates can now have up to 128 channels
- The following Modbus function codes are now supported: FC01 (0x01) / FC03 (0x03) / FC04 (0x04) / FC15 (0x0F) / FC16 (0x10)
New HTML based visualization:
- Application runs in a browser tab
- Widget library 
- 50 dashboards for placing information
New Bender Modbus image V2 has been integrated. Necessary to map the new address structure to Modbus and to provide all data correctly. 
Mapping tables for Modbus, PROFIBUS and SNMP 
BMS devices will now always be displayed with at least 12 channels 
Reset to factory settings integrated
SNMP traps are now supported 
Excel export/import for: Individual texts / Modbus device integration / Alarm addresses
CP700: New display application with new addressing scheme
Slovak has been added as language
NGRM500 support

.................................................................................

V2.36
Date: July 2019 | Device: COM465IP / COM465DP / CP700

Bugfixing Modbus TCP communication
Bugfixing Email function

.................................................................................

V2.35
Date: February 2019 | Device: COM465IP / COM465DP / CP700

isoHR1685DW-9 support
Bugfixing PEMxxx
Bugfixing BMSe communication

.................................................................................

V2.34
Date: December 2018 | Device: COM465IP / COM465DP / CP700

PEM353 support
RCMB13x support
RCMB301 support
MRCDB30x support
isoPV1685RTU-4 (MB / BMS) support
isoLR1685DP-3 support
isoHV1685D-4 support
isoHR1685D-9 support
SMI473-12 support
Bugfixing 

.................................................................................

V2.31
Date: January 2018 | Device: COM465IP / COM465DP / CP700

Bugfixing PEMxxx: Presentation ot the data recorder 

.................................................................................

V2.30
Date: December 2017 | Device: COM465IP / COM465DP / CP700

Note: Connected PRC487 (up to V1.90) perform a restart only after a restart of the COMTRAXX device!
      To completely solve this problem, the PRC487 must be updated to the latest version.

The management and creation of Modbus and virtual devices has been integrated into the HTML interface 
A Modbus documentation can be created which contains the complete BCOM-subsystem information (BCOM-subsystem in which the COMTRAXX® device is located) accessible via Modbus  
Data recorders of all PEMxxx devices have been integrated into the HTML interface
System monitoring can be set that enables e-mail notification
The bus overview in the HTML interface now shows on which COMTRAXX® device the user currently is and which functional modules this device has
The upload interval to POWERSCOUT® is now configurable from between 1…60 minutes
Tables can be sorted and filtered
System documentation can now be created that includes all device parameters
Bugfixing 

.................................................................................

V2.23
Date: July 2017 | Device: COM465IP / COM465DP / CP700

Bugfixing BCOM communication

.................................................................................

V2.22
Date: June 2017 | Device: COM465IP / COM465DP / CP700

COM465DP: Bugfixing Profibus communication

.................................................................................

V2.21
Date: April 2017 | Device: COM465IP / COM465DP / CP700

Communication and data exchange between the COMTRAXX® devices has been completely reworked (no more limits for max. configuration in a system)  
Device documentation: All device parameters and informations as .pdf file
Backup can be generated and imported from all devices: All settings and configuration files
Article and serial number in the bus overview under list view
The layout of the e-mail has been reworked
Bugfixing 

.................................................................................

V2.12
Date: September 2016 | Device: COM465IP / COM465DP / CP700

Data logger and history export to .csv file
Reflection of alarms from virtual devices into the internal BMS bus is possible
iso1685DP-4 support
iso1685P-4 support
Bugfixing 

.................................................................................

V2.10
Date: June 2016 | Device: COM465IP / COM465DP / CP700

Systemwide access to all integrated devices from every gateway (max. configuration for a system: 8 Gateways and 800 Devices) 
Configuration of individual texts now only on device menus
Same individual texts for subsystems in the whole system
Same individual texts for BCOM devices in the whole system
Individual texts for data loggers
3rd party devices: Byte an Word Order settable
Reports only in the new user Interface (HTML5)
E-Mail: Languages per profile settable
Function module E Virtual devices: 100x16 Channels (without Function module: 1x16 Channels)
Function module F 3rd party devices: 1600 Datapoints (without Function module: 50 Datapoints)
Increase max. number of channels for the notification via Email: 5000
Access to POWERSCOUT®
Bugfixing 
Improved performance

.................................................................................

V2.06
Date: March 2016 | Device: COM465IP / COM465DP / CP700

PEM333: DigIn and DigOut displayed as measurement in the device menu

.................................................................................

V2.05
Date: January 2016 | Device: COM465IP / COM465DP

Correction of RS485 bias voltage if devices is master
Bugfix: BMS log for 1...7 days works again

.................................................................................

V2.04
Date: December 2015 | Device: COM465IP / COM465DP / CP700

PEM575-151 support
iso1685FR-5 support
New BMS commands
New texts
Default BCOM Systemname changed: from BENDER to SYSTEM
CP700 Display: Switchable view List/Grid
CP700 Display: Performance optimization
Bugfixing

.................................................................................

V2.03
Date: November 2015 | Device: COM465IP / COM465DP

New BMS commands
New texts
Bugfixing

.................................................................................

V2.00
Date: September 2015 | Device: CP700

New user Interface (HTML5)
User Interface: parameterization possible also via Display, tablet, …
BCOM integration (iso685)
SNMP walk, single get (V1, V2c, V3: values, alarms)
Email: TLS support
30 Data loggers à 10.000 entries
3rd party devices: 50 data points from any Modbus device
Virtual devices: 1 Device x 16 Channels