Signal converter SMO482-12 for messages from Bender devices with BENDER BMS bus to relay contacts.

Supply voltage: AC 230 V

Outputs:           	
12 relay outputs as changeover contacts, 
Operating mode can bet set from N/O operation to N/C operation. 
Making capacity AC/DC 5 A,
Alarm address/channel factory-set
Programmable

Interface: RS485/BMS bus

The enclosure is suitable for:
- Installation into standard distribution panels acc. to DIN 43871
- DIN rail mounting acc. to DIN EN 60715
- Screw mounting

Manufacturer: 		
Bender GmbH & Co.KG
Londorfer Str. 65   
35305 Gruenberg

Type: SMO482-12